**Read me first**

This example works with a post-processor for the WoodWOP v6.1 Homag Group AG CAM system. The final CNC program is generated in MPR format. The “Leg of Table.ipt” component carries a program that generates a WoodWOP MPR program that calls “Recess processing for Leg.mpr” macro. The macro perfoms specific recess for leg mounting in the Table Top part of furniture. The program demonstrates the case when component caries call of macro which performs complicated CNC processing. Also JS Macro passes parameters of “Leg of Table.ipt” to macro and it allows o adjust form of recess. The recess processing uses “Recess processing for Leg.mpr”. You will find this Woodwop Macro next to “Leg of Table.ipt” component. Copy the Macro to "Makros” subdirectory to the directory where all Woodwop components (macros) are stored. In the standard installation of Woodwop all Macros are placed "C:\MACHINE1\Control \c1\data\cnc\ML4\Macros\" in the path.

